<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">\section{FD-SOI for Quantum Computing}
Right now we're in the NISQ era (Noisy Intermediate-Scale Quantum).
on Silicon, we use quantum dot technology.
It works at \SI{4}{\kelvin} and uses a single electron transistor (SET).

\subsection{Electron Spin Resonance}
Use a fix magnetic field and a microwave to flip the spin of the electron.
\begin{align}
    E      &amp; = g\mu_B B                                                        \\
           &amp; =h\nu                                                             \\
    B^{ac} &amp; = \frac{e E_{ac} l_{orb}^2 \abs{\derivative{B\perp}{y}}}{E_{orb}}
\end{align}
Then use the ELzerman protocol to read the spin state via the current.
\begin{figure}[H]
    \centering
    \caption{ELzerman protocol}
    \includegraphics[width=.8\textwidth]{imgs/elzerman_protocol.png}
\end{figure}</pre></body></html>